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          乐清市乐宇自动化电气有限公司
                Yueqing Leyu Electric Automation Co., Ltd.


25W Single Output Open Frame Switching Power Supply       PS-25 series
Universal AC input/Full range
Low price and high reliability

Low leakage current<0.5mA

Protection: short circuit/ overload/ over voltage/ over temperature

Cooling by free air convection

100% full-load burning test
2 years warranty

	SPECIFICATIONS
	
	
	
	

	OUTPUT
	

	MODEL
	PS-25-5
	PS-25-12
	PS-25-15
	PS-25-24

	DC Voltage
	5V
	12V
	15V
	24V

	Rated Current
	5A
	2.1A
	1.7A
	1A

	Rated Power
	25W
	25.2W
	25.5W
	24W

	Ripple & Noise
	80mV
	100mV
	100mV
	240mV

	Voltage Tolerance
	±2%
	±2%
	±2%
	±2%

	Line regulation
	±0.5%
	±0.3%
	±0.3%
	±0.2%

	Load regulation
	±2%
	±1%
	±1%
	±0.5%

	Setup, Rise Time
	200ms,20ms/230VAC    200ms,30ms/115VAC at full load

	Hold Up Time
	100ms/230VAC        20ms/115VAC at full load

	
	

	INPUT
	

	Voltage Range
	85-264VAC   47-63Hz; 120-370VDC

	Efficiency
	74%
	78%
	78%
	79%

	Inrush Current
	Cold-start current 36A

	Leakage current
	<0.5mA/240VAC

	
	

	PROTECTION
	

	Over Load
	Above 105% rated output power

	
	Protection type: hiccup mode, recovery automatically after fault condition is removed

	
	

	ENVIRONMENT
	

	Working Temp., Humidity
	-10℃~+60℃; 20%~90% RH

	Vibration
	10~500Hz,2G 10min,/1cycle,Period for 60min,Each X, Y, Z axes

	
	

	SAFETY
	

	Withstand Voltage
	I/P-O/P: 3KVAC   I/P-FG: 2KVAC   O/P-FG: 0.5KVAC

	Isolation Resistance
	I/P-O/P, I/P-FG, O/P-FG: 100M Ohms/500VDC/25℃/70% RH

	
	

	STANDARD
	

	Safety Standard
	Meet UL60950-1.TUV EN60950-1 approved

	EMC Standard
	EN5022 CLASS B EN61000-3-2-3, EN61000-4-2.3.4.5, light industry level criteria A

	
	

	OTHERS
	

	Dimension
	107*61*28mm(L*W*H)

	Weight
	0.14Kg

	Packing
	96PCS/15Kg/1.3CUFT
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AC nput Connecto (1) : Yolex 4179163 or eqivalent

DC Output Comnector (2 : Nolex 41751-04 or equivalent
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