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          乐清市乐宇自动化电气有限公司
                Yueqing Leyu Electric Automation Co., Ltd.


5000W Single Output switching power supply    SV-5000 series
Features: 
·High efficiency, high reliability
100% full load burn-in test
Protection: Short circuit/ Over load / Over voltage
1 year warranty
	SPECIFICATIONS

	OUTPUT
	

	Model
	SV-5000-30
	SV-5000-40
	SV-5000-110

	DC Voltage
	30V
	40V
	110V

	Rated Current
	167.0A
	120.0A
	45.0A

	Current Range
	0-167.0A
	0-120.0A
	0-45.0A

	Ripple & Noise
	0.50%
	0.50%
	0.50%

	Voltage Adj. Range
	0-30V
	0-40V
	0-110V

	Setup&Rise Time
	100ms,50ms at full load

	Hold Up Time
	20ms at full load

	INPUT
	

	Voltage Range
	AC220V±20%   47～63HZ

	AC Current
	3.2A/115V   1.6A/230V

	Efficiency
	86%
	87%
	89%

	Inrush Current
	40A/230V

	Leakage Current
	<0.5MA/230VAC

	PROTECTION
	

	Over Load
	110～150%  

	
	Protection type: Shut down o/p voltage, re-power on to recover

	Over Voltage
	115～150%  

	
	Protection type: Shut down o/p voltage, re-power on to recover

	SAFETY
	

	Withstand Voltage
	I/P-O/P:1.5KVAC/1min      I/P-F/G:1.5KVAC/1min                        

	Isolation Resistance
	 O/P-F/G:0.5KVAC /1min

	Size
	 500*500*150mm

	NOTE
	

	1.All parameters NOT specially mentioned are measured at 230VAC input, rated load and 25℃ of ambient temperature.
2.Ripple & noise are measured at 20MHz of bandwidth by using a 12” twisted pair-wire terminated with a 0.1μ & 47μ parallel capacitor.
3.Tolerance: includes set up tolerance, line regulation and load regulation
4.The power supply is considered a component which will be installed into a final equipment. The final equipment must be re-confirmed that it still meets EMC directives.

	

	

	



